Blue Box                               courtesy of the Jolly Roger

To quote Karl Marx, blue boxing has always been the most noble form of
phreaking. As opposed to such things as using an MCI code to make a free
fone call, which is merely mindless pseudo-phreaking, blue boxing
is actual interaction with the Bell System toll network.
It is likewise advisable to be more cautious when blue boxing, but the
careful phreak will not be caught, regardless of what type of switching
system he is under.
In this part, I will explain how and why blue boxing works, as well as
where. In later parts, I will give more practical information for blue
boxing and routing information. To begin with, blue boxing is simply
communicating with trunks. Trunks must not be confused with subscriber
lines (or "customer loops") which are standard telefone lines. Trunks are
those lines that connect central offices. Now, when trunks are not in
use (i.e., idle or "on-hook" state) they have 2600Hz applied to them. If
they are two-way trunks, there is 2600Hz in both directions. When a trunk
IS in use (busy or "off-hook" state), the 2600Hz is removed from the side
that is off-hook. The 2600Hz is therefore known as a supervisory
signal, because it indicates the status of a trunk; on hook (tone) or
off-hook (no tone). Note also that 2600Hz denoted SF (single frequency)
signalling and is "in-band." This is very important. "In-band" means that
is within the band of frequencies that may be transmitted over normal
telefone lines. Other SF signals, such as 3700Hz are used also. However,
they cannot be carried over the telefone network normally (they are
"out-of-band" and are therefore not able to be taken advantage of as
2600Hz is. Back to trunks. Let's take a hypothetical phone call. You pick
up your fone and dial 1+806-258-1234 (your good friend in Amarillo, Texas).
For ease, we'll assume that you are on #5 Crossbar switching and not in the
806 area. Your central office (CO) would recognize that 806 is a foreign
NPA, so it would route the call to the toll centre that serves you.
[For the sake of accuracy here, and for the more experienced readers,
note that the CO in question is a class 5 with LAMA that uses out-of-band
SF supervisory signalling]. Depending on where you are in the country,
the call would leave your toll centre (on more trunks) to another toll
centre, or office of higher "rank". Then it would be routed to central
office 806-258 eventually and the call would be completed.

            Illustration
A---CO1-------TC1------TC2----CO2----B

A.... you
CO1=your central office
TC1.. your toll office.
TC2.. toll office in Amarillo.
CO2.. 806-258 central office.
B.... your friend (806-258-1234)

In this situation it would be realistic to say that CO2 uses SF
in-band (2600Hz) signalling, while all the others use out-of-band signal-
ling (3700Hz). If you don't understand this, don't worry. I am pointing
this out merely for the sake of accuracy. The point is that while you
are connected to 806-258-1234, all those trunks from YOUR central office
(CO1) to the 806-258 central office (CO2) do *NOT* have 2600Hz on them,
indicating to the Bell equipment that a call is in progress and the trunks
are in use.
Now let's say you're tired of talking to your friend in Amarillo, so you
send a 2600Hz down the line. This tone travels down the line to your
friend's central office (CO2) where it is detected. However, that CO thinks
that the 2600Hz is originating from Bell equipment, indicating to it
that you've hung up, and thus the trunks are once again idle (with 2600Hz
present on them). But actually, you have not hung up, you have fooled the
equipment atyour friend's CO into thinking you have. Thus,it disconnects
him and resets the equipment to prepare for the next call. All this happens
very quickly (300-800ms for step-by-step equipment and 150-400ms for other
equipment). When you stop sending 2600Hz (after about a second), the
equipment thinks that another call is coming towards
--> on hook, no tone -->off hook.
Now that you've stopped sending 2600Hz, several things happen:

1) A trunk is seized.
2) A "wink" is sent to the CALLING end from the CALLED end indicating that
the CALLED end (trunk) is not ready to receive digits yet.
3) A register is found and attached to the CALLED end of the trunk within
about two seconds (max).
4) A start-dial signal is sent to the CALLING end from the CALLED end
indicating that the CALLED end is ready to receive digits.
Now, all of this is pretty much transparent to the blue boxer. All he
really hears when these four things happen is a <beep><kerchunk>. So,
seizure of a trunk would go something like this:

1> Send a 2600Hz
2> Terminate 2600Hz after 1-2 secs.
3> [beep][kerchunk]

Once this happens, you are connected to a tandem that is ready to obey your
every command. The next step is to send signalling information in order to
place your call. For this you must simulate the signalling used by
operators and automatic toll-dialing equipment for use on trunks. There are
mainly two systems, DP and MF. However, DP went out with the dinosaurs, so
I'll only discuss MF signalling. MF (multi-frequency) signalling is the
signalling used by the majority of the inter- and intra-lata network. It is
also used in international dialing known as the CCITT no.5 system.
MF signals consist of 7 frequecies, beginning with 700Hz and separated by
200Hz. A different set of two of the 7 frequencies represent the digits 0
thru 9, plus an additional 5 special keys. The frequencies and uses are as
follows:

Frequencies (Hz)  Domestic    Int'l
-------------------------------------
 700+900             1          1
 700+1100            2          2
 900+1100            3          3
 700+1300            4          4
 900+1300            5          5
1100+1300            6          6
 700+1500            7          7
 900+1500            8          8
1100+1500            9          9
1300+1500            0          0
 700+1700           ST3p       Code 1
 900+1700           STp        Code 1
1100+1700           KP         KP1
1300+1700           ST2p       KP2
1500+1700           ST         ST
 The timing of all the MF signals is a nominal 60ms, except for KP, which
should have a duration of 100ms. There should also be a 60ms silent period
between digits. This is very flexible however, and most Bell equipment will
accept outrageous timings. In addition to the standard uses
listed above, MF pulsing also has expanded usages known as "expanded
inband signalling" that include such things as coin collect, coin return,
ringback, operator attached, and operator attached, and operator
released. KP2, code 11, and code 12 and the ST_ps (STart "primes" all have
special uses which will be mentioned only briefly here.
To complete a call using a blue box once seizure of a trunk has been
accomplished by sending 2600Hz and pausing for the <beep><kerchunk>, one
must first send a KP. This readies the register for the digits that follow.
For a standard domestic call, the KP would be followed by either 7 digits
(if the call were in the same NPA as the seized trunk) or 10 digits (if the
call were not in the same NPA as the seized trunk). [Exactly like dialing
normal fone call]. Following either the KP and 7 or 10 digits, a STart is
sent to signify that no more digits follow. Example of a complete call:

1> Dial 1-806-258-1234
2> wait for a call-progress indication (such as ring,busy,recording,etc.)
3> Send 2600Hz for about 1 second.
4> Wait for about ll-progress indication (such as ring,busy,recording,etc.)
5> Send KP+305+994+9966+ST
The call will then connect if everything was done properly. Note that if a
call to an 806 number were being placed in the same situation, the are code
would be omitted and only KP + seven digits + ST would be sent.
Code 11 and code 12 are used in international calling to request
certain types of operators. KP2 is used in international calling to route a
call other than by way of the normal route, whether for economic or
equipment reasons. STp, ST2p, and ST3p (prime, two prime, and three prime)
are used in TSPS signalling to indicate calling type of call (such as
coin-direct dialing.

It all started here................... RFLAGG